Extra items:

Push Button = Port\_P bit 5

Bit 5 off = button pressed

Port\_PDDR is still sent $1E for stepper motor

INTCR $80 sets edge trigger

INTCR $40 enable IRQ

VECTOR 6 irq\_FUNCTION